# USB might be /dev/ttyACM0
# serial might be /dev/ttyS0
# pps might be /dev/pps0
DEVICES="/dev/ttyS0 /dev/pps0"

# -n means start without a client connection (i.e. at boot)
# -s 115200 is to set baud to 115200
GPSD_OPTIONS="-n -s 115200"

# also start in general
START_DAEMON="true"

# Automatically hot add/remove USB GPS devices via gpsdctl
USBAUTO="true"
